| ManualsContentsPreviousNext |

# Connecting to the USB (Type B) Interface

This section describes how to connect the USB2.0 (Type B) interface cable to the USB2.0 port.

Caution:

Properly shield twisted pair cable (STP cable) must be used for connections to a host computer (and/or peripheral) in order to meet emission limits.

1. Connect the USB2.0 (Type B) interface cable to the USB2.0 port.

   - When connecting the USB interface cable to the standard USB2.0 (Type B) port

   - When connecting the USB interface cable to the USB2.0 (Type B) port on the Gigabit Ethernet board

2. Connect the other end to the USB2.0 port on the host computer.

- This machine does not come with a USB interface cable. Make sure you purchase the appropriate cable for the machine and your computer.

- The USB2.0 interface board is supported by Windows XP/Vista/7, Windows Server 2003/2003 R2/2008/2008 R2, Mac OS X 10.3.3 or higher.

  - When used with Mac OS X 10.3.3 or higher, a transfer speed of USB2.0 is supported.

- For details about installing the printer driver, see "Preparing the Machine", Printer Reference.