| ManualsContentsPreviousNext |

# When Y1 - Y3 is displayed

“Y1”, “Y2”, and “Y3” indicate a paper jam has occurred in the following optional trays:

- “Y1”: Tray 2

- “Y2”: Tray 3

- “Y3”: Tray 4

The following example explains how to remove a paper jam in tray 2.

The same procedure can be used for paper in trays 3 and 4.

1. Carefully pull out tray 2 until it stops.

2. Remove the misfed paper, and then carefully push tray 2 fully in.

3. Push the button on the right side of the machine to open the front cover.

4. Close the front cover.