| ManualsContentsPreviousNext |

# Margin Adjustment

Copies originals leaving a binding margin.

1. Press [Edit / Stamp].

2. Make sure that [Margin Adj.] is selected. If [Margin Adj.] is not selected, press [Margin Adj.].

3. Specify a binding margin for the front side pages.

4. Specify a binding margin for the back side pages. Then press [OK].

   If you do not need to specify the margins for the back side pages, press [OK].

- To change the value you entered, press [], [], [] or [], or press [Clear], and then specify a new value.

- Press [] and [] to set the top or bottom position. Press [] and [] to set the left or right position.

- You can set the binding margin up to 30 mm (1.2 inches) in 1 mm (0.1 inches) increments.

- Margin on the back side of the page is valid when 1 Sided 2 Sided or Combine 2 Sides is selected.

- You can change the settings for Margin Adjustment under Edit in User Tools. For details about Edit, see “Edit”.

- If you set a binding margin that is too wide, part of the image may not be copied.

- When making copies in Combine mode, the binding margin is added to the copies after the combination is finished.

- Edit