ManualsContentsPreviousNext
Settings

# Moving the Machine

This section describes precautions when moving the machine.

Be sure to check the following points:

- The power switch is turned off.

- The power cord is unplugged from the wall outlet.

- The interface cable is unplugged from the machine.

If any external options are attached, remove them.

See the relevant sections in this manual and reverse the steps to remove options.

Lift the machine by the inset grips on its sides.

At least four people are needed to lift the machine.

Move the machine horizontally to the place where you want to install it.

If you removed options, reattach them.

For details, see the relevant sections in this manual.

- Be sure to move the machine horizontally. To prevent toner from scattering, move the machine slowly.