| ManualsContentsPreviousNext |

# Setting Items of IEEE 802.1X for Wireless LAN

1. Log in to Web Image Monitor in the administrator mode.

2. In the menu area, click [Configuration].

3. Under "Security", click [IEEE 802.1X].

4. In "User Name", enter the user name set in the RADIUS server.

5. Enter the domain name in "Domain Name".

6. Select "EAP Type". Configurations differ according to the EAP Type.

   EAP-TLS

   - Make the following settings according to the operating system you are using:

     - Select [On] or [Off] in "Authenticate Server Certificate".

     - Select [On] or [Off] in "Trust Intermediate Certificate Authority".

     - Enter the host name of the RADIUS server on "Server ID".

     - Select [On] or [Off] in "Permit Sub-domain".

   LEAP

   - Click [Change] in "Password", and then enter the password set in the RADIUS server.

   EAP-TTLS

   - Click [Change] in "Password", and then enter the password set in the RADIUS server.

   - Click [Change] in "Phase 2 User Name", and then enter the user name set in the RADIUS server.

   - Select [CHAP], [MSCHAP], [MSCHAPv2], [PAP], or [MD5] in "Phase 2 Method".

     Certain methods might not be available, depending on the RADIUS server you want to use.

   - Make the following settings according to the operating system you are using:

     - Select [On] or [Off] in "Authenticate Server Certificate".

     - Select [On] or [Off] in "Trust Intermediate Certificate Authority".

     - Enter the host name of the RADIUS server in "Server ID".

     - Select [On] or [Off] in "Permit Sub-domain".

   PEAP

   - Click [Change] in "Password", and then enter the password set in the RADIUS server.

     If [TLS] is selected for "Phase 2 Method", you do not need to specify a password.

   - Click [Change] on "Phase 2 User Name", and then enter the user name set in the RADIUS server.

   - Select [MSCHAPv2] or [TLS] in "Phase 2 Method".

     When you select [TLS], you must install "IEEE 802.1X Client Certificate".

   - Make the following settings according to the operating system you are using:

     - Select [On] or [Off] in "Authenticate Server Certificate".

     - Select [On] or [Off] in "Trust Intermediate Certificate Authority".

     - Enter the host name of the RADIUS server on "Server ID".

     - Select [On] or [Off] in "Permit Sub-domain".

7. Click [OK].

8. `"Updating..."` appears. Wait for about one or two minutes, and then click [OK].

9. In the menu area, click [Configuration].

10. Under "Interface", click [Wireless LAN Settings].

11. Select [Wireless LAN] in "LAN Type".

12. Select [Infrastructure Mode] in "Communication Mode".

13. Enter the alphanumeric characters (a-z, A-Z, or 0-9) in [SSID] according to the access point you want to use.

14. Select [WPA] in "Security Method".

15. Select [TKIP] or [CCMP (AES)] in "WPA Encryption Method" according to the access point you want to use.

16. Select [WPA] or [WPA2] in "WPA Authentication Method".

17. Click [OK].

18. `"Updating..."` appears. Wait for about one or two minutes, and then click [OK].

19. Click [Logout].

20. Quit the Web Image Monitor.

- If there is a problem with settings, you might not be able to communicate with the printer. To identify the problem, print a network summary.

- If you cannot identify the problem, reset the printer interface to normal, and then repeat the procedure from the beginning.