| ManualsContentsPreviousNext |

# Wireless LAN

This section lists the settings required for delivering data to the network with a wireless LAN connection.

For details about how to specify the settings, see "Interface Settings" and "File Transfer".

Menu | User Tool | Setting Requirements
--- | --- | ---
Interface Settings/Network | Machine IPv4 Address | Necessary
Interface Settings/Network | IPv4 Gateway Address | As required
Interface Settings/Network | Machine IPv6 Address | As required
Interface Settings/Network | IPv6 Gateway Address | As required
Interface Settings/Network | IPv6 Stateless Address Autoconfiguration | As required
Interface Settings/Network | DNS Configuration | As required
Interface Settings/Network | DDNS Configuration | As required
Interface Settings/Network | IPsec | As required
Interface Settings/Network | Domain Name | As required
Interface Settings/Network | WINS Configuration | As required
Interface Settings/Network | Effective Protocol | Necessary
Interface Settings/Network | LAN Type | Necessary
Interface Settings/Network | Permit SNMPv3 Communication | As required
Interface Settings/Network | Permit SSL / TLS Communication | As required
Interface Settings/Network | Host Name | As required
Interface Settings/Wireless LAN | Communication Mode | Necessary
Interface Settings/Wireless LAN | SSID Setting | As required
Interface Settings/Wireless LAN | Ad-hoc Channel | As required
Interface Settings/Wireless LAN | Security Method | As required
File Transfer | Delivery Option | Necessary
File Transfer | Fax RX File Transmission | As required
File Transfer | Scanner Resend Interval Time | As required
File Transfer | Number of Scanner Resends | As required

- For the Effective Protocol setting, check that the protocol you want to use is set to [Active].

- [Wireless LAN] and [LAN Type] are displayed when the wireless LAN board is installed. When both Ethernet and wireless LAN are connected, the selected interface takes precedence.

- If Delivery Option is set to [On], check that IPv4 Address is specified.

- Interface Settings

- File Transfer