ManualsContentsPreviousNext
Settings

# ipv6

Use the "ipv6" command to display and configure the IPv6 settings.

View Setting

`msh> ipv6`

IPv6 stateless address

`msh> ipv6 stateless {on|off}`

If "on" is selected, IPv6 requests information required for maintaining stateful connection to the router for as long as the printer power is turned on. This setting allows information from the router to be obtained constantly, and periodically refreshes the effective period of the stateless address.