ManualsContentsPreviousNext
Settings

# Windows Vista, Windows Server 2008 - WSD port

Quit all applications currently running.

On the [Start] menu, click [Network].

The [Network] window appears, and the device search begins automatically.

Right-click the machine's icon, and then click [Install].

If the [User Account Control] dialog box appears, click [Continue].

The [Found New Hardware] dialog box appears.

Click [Locate and install driver software (recommended)].

If the [User Account Control] dialog box appears, click [Continue].

Click [Browse my computer for driver software (advanced)].

Insert the provided CD-ROM into the computer's CD-ROM drive.

If the [AutoPlay] dialog box appears, click the [Close] button.

Click [Browse...], and then specify a location for the printer driver.

If the CD-ROM drive is D, the source files of the printer driver are stored in the following locations:

- PCL 5e

  D:\x86 or X64\DRIVERS\PCL5e\XP_VISTA or X64\(Language)\DISK1

- PCL 6

  D:\x86 or X64\DRIVERS\PCL6\XP_VISTA or X64\MUI\DISK1

- PostScript 3

  D:\x86 or X64\DRIVERS\PS\XP_VISTA or X64\MUI\DISK1

The PCL 6 printer driver is installed in the language specified by your operating system.

Click [Next].

If the [Windows can't verify the publisher of this driver software] message appears, click [Install this driver software anyway].

Click [Close].

If installation is successful, the icon of the printer connected to the WSD port is added to the [Printers] window.

- The port name that follows "WSD" uses random character strings. It cannot be changed freely.

- To stop installation of the selected driver, click [Cancel] before the installation is complete. When re-installing the WSD Port, right-click the machine's icon in the [Network] window, and then click [Uninstall].