| ManualsContentsPreviousNext |

# SUB Code Transfer Report

You can check the results of transmission to Receiving Stations. The machine prints this report when it has finished transmitting to Receiving Stations.

- You can select whether the SUB Code Transfer Report be automatically printed using the User Parameter (switch 04, bit 1) in the Facsimile Features menu.

- You can set whether a portion of the original image is printed on the report with the User Parameter (switch 04, bit 7) in the Facsimile Features menu.

- For details about Parameter Setting, see “Parameter Settings”.

- “Unprogrammed” indicates the document could not be sent because the end receiver is not programmed.

- “--” indicates that the e-mail or Internet Fax document was sent to the mail server programmed in this machine.

- For the maximum number of destinations you can register in a group, see “Maximum Values”.

- Parameter Settings

- Maximum Values