ManualsContentsPreviousNext
Settings

# Removing Jammed Paper

This section describes how to locate and remove jammed paper.

| The inside of the machine could be very hot. Do not touch the parts with a label indicating the "hot surface." Otherwise, an injury might occur.

| Some of this machine's internal components get very hot. For this reason, take care when removing misfed paper. Not doing so could result in burns.

- When clearing misfeeds, do not turn off the operation switch. If you do, your copy settings will be lost.

- To prevent misfeeds, do not leave any torn scraps of paper inside the machine.

- Contact your service representative if misfeeds occur frequently.

- When removing jammed sheets, take care to touch only those areas explicitly indicated in the manual.

- Do not remove the fusing unit. Doing so will result in loss of print quality.

- If the error message remains displayed even after you remove misfed paper, open and close the front cover.

- If a detailed removal instruction appears on the right of the screen, follow it.

- You can also use the procedure indicated in [System Status] to remove jammed paper.

Related topics

Locating Jammed Paper
When A1 is displayed
When A2 is displayed
When B is displayed
When C is displayed
When P is displayed
When R is displayed (Type 3 Only)
When Y1 - Y3 is displayed
When Z1 - Z2 is displayed