| ManualsContentsPreviousNext |

# Changing the port settings for SmartDeviceMonitor for Client

Follow the procedure below to change the SmartDeviceMonitor for Client settings, such as TCP/IP timeout.

Windows XP, Windows Server 2003/2003 R2:

1. On the [Start] menu, click [Printers and Faxes].

   The [Printers and Faxes] window appears.

2. Click the icon of the printer you want to use. On the [File] menu, click [Properties].

3. Click the [Ports] tab, and then click [Configure Port...].

   The [Port Configuration] dialog box appears.

Windows Vista, Windows Server 2008:

1. On the [Start] menu, click [Control Panel].

   The [Control Panel] window appears.

2. Click [Printer] in "Hardware and Sound".

   The [Printers] window appears.

3. Right-click the icon of the printer you want to use, and then click [Properties].

4. Click the [Ports] tab, and then click [Configure Port...].

   The [Port Configuration:] dialog box appears.

Windows 7, Windows Server 2008 R2:

1. On the [Start] menu, click [Devices and Printers].

   The [Devices and Printers] window appears.

2. Right-click the icon of the printer you want to use, and then click [Printer properties].

3. Click the [Ports] tab, and then click [Configure Port...].

   The [Port Configuration] dialog box appears.

- User, proxy, and timeout settings can be configured for IPP.

- For details about these settings, see "Using the SmartDeviceMonitor for Client Port", or SmartDeviceMonitor for Client Help.

- Using the SmartDeviceMonitor for Client Port