ManualsContentsPreviousNext
Settings

# Using the Standard TCP/IP Port

This describes how to install the PCL or PostScript® 3TM printer driver using the Standard TCP/IP port.

- Manage Printers permission is required to install the driver. Log on as an Administrators group member.

- In an IPv6 environment, you cannot use the Standard TCP/IP Port. Use the SmartDeviceMonitor for Client port.

- You can install the printer driver from the CD-ROM provided with this machine or download it from the manufacturer's Web site.

Related topics

Installing the PCL printer driver
Installing the PostScript 3 printer driver