ManualsContentsPreviousNext
Settings

# Loading Orientation-Fixed Paper or Two-Sided Paper

This section describes loading paper that has a specified orientation and printing side (such as letterhead paper).

Orientation-fixed (top to bottom) or two-sided paper (for example, letterhead paper, punched paper, or copied paper) might not print correctly, depending on how the originals and paper are placed. Set [Letterhead Setting] to [Yes] in [Input / Output] under [Copier / Document Server Features], and then place the original and paper as shown below. For details about Letterhead Setting, see “Copier and Document Server Features”, Copy and Document Server Reference. For details about printing with the printer function, see “Printing on Orientation-Fixed or Two-Sided Paper”, Printer Reference.

Original Orientation

Exposure glass | ADF
--- | ---
| Copy Scanner |  |

Paper Orientation