| ManualsContentsPreviousNext |

# Immediate Transmission

Immediate Transmission is possible with standard fax transmission and IP-Fax transmission.

- Internet Fax, e-mail transmission and folder transmission are performed using Memory Transmission, which automatically starts transmission after storing documents in memory. If you switch the type of transmission to them while the machine is in Immediate Transmission mode, the transmission mode is automatically switched to Memory Transmission.

- Group cannot be used for Immediate Transmission. You cannot send the same document to multiple destinations (broadcasting). If you specify broadcast or transmission for a group, the machine changes automatically to Memory Transmission.

1. Press [Immed. TX].

2. Place the original into the ADF.

3. Select the scan settings you require.

   For details about the scan settings, see “Scan Settings”.

4. Using the number keys or a Destination key, specify a destination.

   If you make a mistake, press the [Clear/Stop] key, and then enter the correct number.

   For details about specifying a destination, see “Specifying a Destination”.

5. Press the [Start] key.

   The machine dials a destination.

- Documents are not stored in memory.

- Scan Settings

- Specifying a Destination

Related topics

Sending originals using the exposure glass (Immediate Transmission)