ManualsContentsPreviousNext
Settings

# Using AutoNet

If the machine IPv4 address is not automatically assigned by the DHCP server, a temporary IP address starting with 169.254 and not used on the network can be automatically selected by the machine.

- The IP address assigned by the DHCP server is given priority over that selected by AutoNet.

- You can confirm the current IPv4 address on the configuration page.

- When AutoNet is running, the NetBIOS name is not registered on the WINS server.

- The machine cannot communicate with devices that do not have the AutoNet function. However, this machine can communicate with Macintosh computers running Mac OS X 10.2.3. or higher.