ManualsContentsPreviousNext
Settings

# To add new receiver

Use Web Image Monitor to add a new destination to the Address Book.

Start a Web browser.

Enter “http://(IPv4 address, IPv6 address or host name of this machine)/” in the address bar.

The top page of Web Image Monitor is displayed.

Click [Login], and then enter the Administrator's name and password.

Click [Address Book] in the left pane.

The Address Book is displayed.

Click [Add User].

The [Add User] page appears.

Enter the registration number, name, and e-mail address, then set the necessary properties.

You can set the Internet Fax data format after entering the e-mail address.

Click [Full Mode] under [Internet Fax Data Format], and set the properties according to the receiver's properties.

If you change the mode to “Simple Mode”, you cannot set machine properties.

Click [OK] at the upper or lower left of the screen.

To cancel the setting, click [Cancel] at the upper or lower left of the screen.

The Address Book is displayed.

Close the Web browser.