| ManualsContentsPreviousNext |

# Programming Destination Information from Web Browser

If the receiving machine is compliant with T.37 full mode Internet Fax, you can program the receiver's properties from Web Image Monitor.

You can program the following properties:

- Compression Type

- Paper size

- Resolution

- For a detailed description, see Web Image Monitor Help.

- For details about the T.37 full mode, see “T.37 Full Mode”.

- When a receiver that is programmed as full mode in the Address Book returns a Reception Notice e-mail, the contents of the newly received e-mail overwrite the existing information.

- T.37 Full Mode

Related topics

To edit machine properties already programmed
To add new receiver