| ManualsContentsPreviousNext |

# On Hook Dial

The On Hook Dial function allows you to dial while listening to the tone from the internal speaker.

You can send a fax checking the connection.

- This function is not available for Internet Fax, IP-Fax, and transmission to e-mail/folder destinations.

1. Place the original, and then select the scan settings you require.

2. Press [On Hook].

   You will hear a low tone from the internal speaker.

   If you want to cancel this operation, press [On Hook] again.

3. Dial.

   The machine immediately dials the destination.

   If you make a mistake, press [On Hook] or the [Clear Modes] key, and then try again.

4. When the line is connected and you hear a high-pitched tone, press the [Start] key.

5. Press [Start TX].

   Transmission starts.

   If you want to cancel a transmission, press the [Clear/Stop] key, and then remove the originals.

   After transmission, the standby display appears.

- This function is unavailable in some countries.

- To select a destination from the Address Book, see “Using the Address Book to Specify Destinations”.

- Press [Vol...] to display the Adjust Sound Volume screen, and then press [Louder] or [Lower] to adjust the volume of the on-hook sound. The volume can also be preprogrammed in the Facsimile Features menu.

- If you have an external telephone on the fax machine, you can speak with the other party when you hear a voice. If you hear a voice before pressing the [Start] key, pick up the external telephone and tell the receiver you want to send a fax document (ask them to switch to facsimile mode).

- The Facsimile Features menu contains the On Hook Mode Release Time setting, which allows you to specify the time after which On Hook mode is deactivated. See “General Settings”.

- Using the Address Book to Specify Destinations

- General Settings