| ManualsContentsPreviousNext |

# Specifications for the Main Unit

Configuration:

Desktop

Original scanning:

One-dimensional solid scanning system through CCD

Copy process:

Laser beam scanning and electro-photographic printing

Development:

Monocomponent Nonmagnetic Development System

Fusing:

Heating roll pressure system

Resolution:

- Scanning:

  Exposure glass: 600 × 600 dpi

  ADF: 600 × 300 dpi

- Printing:

  600 × 600 dpi, 1,200 × 600 dpi

Exposure glass:

Stationary original exposure type

Original reference position:

Rear left corner

Warm-up time (23 °C (73 °F), rated voltage):

20 seconds or less

Originals:

Sheet/book/objects

Maximum original size:

A4, 81/2 × 11

Paper size:

- Tray 1:

  A4, A5, A6, B5 JIS, B6 JIS, 81/2 × 14, 81/2 × 13, 81/2 × 11, 81/4 × 13, 8 × 13, 71/4 × 101/2, 51/2 × 81/2, 16K

  41/8 × 91/2, 37/8 × 71/2, C5 Env, C6 Env, DL Env

- Tray 1 (custom size):

  Vertical: 140.0 356.0 mm (5.52 14.01 inches)

  Horizontal: 98.0 216.0 mm (3.86 8.50 inches)

- Bypass tray:

  A4, A5, A6, B5 JIS, B6 JIS, 81/2 × 14, 81/2 × 13, 81/2 × 11, 81/4 × 13, 8 × 13, 71/4 × 101/2, 51/2 × 81/2, 16K

  41/8 × 91/2, 37/8 × 71/2, C5 Env, C6 Env, DL Env

- Bypass tray (custom size):

  Vertical: 140.0 900.0 mm (5.52 35.43 inches)

  Horizontal: 64.0 216.0 mm (2.52 8.50 inches)

- Duplex:

  A4, A5, B5 JIS, B6 JIS, 81/2 × 14, 81/2 × 13, 81/2 × 11, 81/4 × 13, 8 × 13, 71/4 × 101/2, 51/2 × 81/2, 16K

- Duplex (custom size):

  Vertical: 160.0 356.0 mm (6.30 14.01 inches)

  Horizontal: 98.0 216.0 mm (3.86 8.50 inches)

Paper weight:

- Tray 1 and bypass tray: 52 220 g/m2 (14 lb. Bond 80 lb. Cover)

- Duplex: 60 163 g/m2 (16 lb. Bond 90 lb. Index)

For details about and recommendations concerning thick paper, see “Thick Paper”.

Non-reproduction area (Copier):

- Leading edge: 1 5 mm (0.04 0.20 inches)

- Left and right: 0.5 3.5 mm (0.02 0.14 inches)

- Trailing edge: 0 4 mm (0.00 0.16 inches)

First copy/print time:

- (mainly Europe and Asia)

  - Types 1 and 3: 8.6 seconds

  - Type 2: 8.4 seconds

- (mainly North America)

  - Types 1 and 3: 8.4 seconds

  - Type 2: 8.5 seconds

(A4, 81/2 × 11, 100% reproduction, feeding from tray 1, on the exposure glass)

Copy/print speed:

- Type 1: 45 sheets/minute (A4), 47 sheets/minute (81/2 × 11)

- Types 2 and 3: 50 sheets/minute (A4), 52 sheets/minute (81/2 × 11)

Reproduction ratio:

- (mainly Europe and Asia)

  Preset reproduction ratios:

  - Enlargement: 200%, 141%

  - Full size: 100%

  - Reduction: 93%, 71%, 50%

- (mainly North America)

  Preset reproduction ratios:

  - Enlargement: 155%, 129%

  - Full size: 100%

  - Reduction: 93%, 78%, 65%

- Zoom:

  - ADF: From 25 to 200% in increments of 1%

  - Exposure glass: From 25 to 400% in increments of 1%

Maximum continuous copy run:

999 sheets

Paper capacity (75 g/m2, 20 lb. Bond):

- Tray 1: 550 sheets

- Bypass tray: 100 sheets

Stack capacity for Internal tray 1 (80 g/m2, 21 lb. Bond):

500 sheets

Power requirements:

- (mainly Europe and Asia)

  220 240 V, 50/60 Hz, 7 A

- (mainly North America)

  120 127 V, 60 Hz, 12 A

Power consumption:

- Main unit only

  | Type 1 | Type 2 | Type 3
  --- | --- | --- | ---
  Stand-by | About 200 W About 194 W | About 200 W About 197 W | About 160 W About 159 W
  During printing | About 843 W About 863 W | About 869 W About 892 W | About 833 W About 858 W
  Maximum | 1,500 W | 1,500 W | 1,500 W

- Complete system

  | Type 1 | Type 2 | Type 3
  --- | --- | --- | ---
  Maximum | 1,500 W | 1,500 W | 1,500 W

  - The complete system of types 1 and 3 consists of the main unit, Gigabit Ethernet, fax unit, two paper feed units, and paper feed unit with the casters.

  - The complete system of type 2 consists of the main unit, Gigabit Ethernet, two paper feed units, and paper feed unit with the casters.

Dimensions (W × D × H up to ADF):

- Types 1 and 2: 460 × 510 × 686mm (18.2 × 20.1 × 27.0 inches)

- Type 3: 460 × 615 × 686mm (18.2 × 24.3 × 27.0 inches)

Noise emission:

- Sound power level:

  - Main unit only

    | Type 1 | Type 2 | Type 3
    --- | --- | --- | ---
    Stand-by | Less than 41.8 dB(A) | Less than 41.8 dB(A) | Less than 41.8 dB(A)
    Copying | Less than 72.0 dB(A) | Less than 73.0 dB(A) | Less than 73.0 dB(A)

  - Complete system

    | Type 1 | Type 2 | Type 3
    --- | --- | --- | ---
    Stand-by | Less than 41.8 dB(A) | Less than 41.8 dB(A) | Less than 41.8 dB(A)
    Copying | Less than 72.0 dB(A) | Less than 73.0 dB(A) | Less than 73.0 dB(A)

- Sound pressure level:

  - Main unit only

    | Type 1 | Type 2 | Type 3
    --- | --- | --- | ---
    Stand-by | Less than 35.8 dB(A) | Less than 35.8 dB(A) | Less than 35.8 dB(A)
    Copying | Less than 66.0 dB(A) | Less than 67.0 dB(A) | Less than 67.0 dB(A)

  - Complete system

    | Type 1 | Type 2 | Type 3
    --- | --- | --- | ---
    Stand-by | Less than 35.8 dB(A) | Less than 35.8 dB(A) | Less than 35.8 dB(A)
    Copying | Less than 66.0 dB(A) | Less than 67.0 dB(A) | Less than 67.0 dB(A)

    - Sound power level and sound pressure level are actual values measured in accordance with ISO 7779.

    - Sound pressure level is measured from the position of the bystander.

    - The complete system consists of the main unit, two paper feed units, and paper feed unit with the casters.

Weight:

- Type 1: 45 kg (99.2 lb.) or less

- Type 2: 47 kg (103.7 lb.) or less

- Type 3: 52 kg (114.7 lb.) or less

- Thick Paper

Related topics

Auto Document Feeder
Document Server
Internal Tray 2 (Type 2 Only)
Finisher (Type 3 Only)