| ManualsContentsPreviousNext |

# Confirming Transmission Results by E-mail

Use this function to confirm the transmission results by sending an e-mail notification to the specified destination.

- Register the e-mail address of the destination for e-mail notification in the destination list in advance.

1. Place the original, and then select the scan settings you require.

2. Specify the sender.

   For details, see “Sender Settings”.

3. Press [TX Mode].

4. Press [E-mail TX Results].

5. Select the destination of notification, and then press [OK].

   If you make a mistake, before pressing [OK], press [Clear] or press the selected Destination key again to turn the highlight off.

   [E-mail TX Results] gets highlighted and the destination of notification selected appears.

6. Press [OK].

   The standby display appears.

   To check the settings, press [TX Mode].

7. Specify a destination, and then press the [Start] key.

- You can program one of the Quick Operation keys with operations for this function. Using the Quick Operation Key allows you to omit steps 3 and 6. For details about Quick Operation Key, see “General Settings”.

- Sender Settings

- General Settings