| ManualsContentsPreviousNext |

# hostname

Use the "hostname" command to change the printer name.

View settings

`msh> hostname`

IPv4 Configuration

`msh> hostname "interface_name" name "printer_name"`

- Enter the printer name using up to 63 alphanumeric characters.

- You cannot use a printer name beginning "RNP" (in either upper or lower case).

- The Ethernet interface and IEEE 802.11 interface will have the same printer name.

- wlan can be specified only when the IEEE 802.11 interface is installed.

- If you do not specify an interface, the Ethernet interface is selected automatically.

Interface name | Interface configured
--- | ---
ether | Ethernet interface
wlan | IEEE 802.11 interface

Initializing the printer name for each interface

`msh>hostname "interface_name" clear name`