ManualsContentsPreviousNext
Settings

# Installing the PostScript 3 printer driver (TCP/IP)

Quit all applications currently running.

Insert the CD-ROM into the CD-ROM drive.

The installer starts.

Select an interface language, and then click [OK].

The printer driver with the selected language will be installed. The English printer driver is installed when the following language is selected: Suomi, Magyar, Cestina, Polski, Portugues, Russian.

Click [PostScript 3 Printer Driver].

Add Printer Wizard starts.

Click [Next >].

Click [Local printer attached to this computer], and then click [Next >].

Click [Create a new port:].

Click [SmartDeviceMonitor for Client 2] in [Type of port:], and then click [Next >].

Click [TCP/IP], and then click [Search].

A list of machines using TCP/IP appears.

Select the machine you want to use, and then click [OK].

Only machines that respond to a broadcast from the computer appear. To use a machine not listed here, click [Specify Address], and then enter the IP address or host name of the machine.

Check that the name of the machine whose driver you want to install is selected, and then click [Next >].

Change the machine name if you want, and then click [Next >].

Select [Yes] to configure the machine as default.

Specify whether or not to share the machine, and then click [Next >].

Specify whether or not to print a test page, and then click [Next >].

Click [Finish].

If the [Hardware Installation] message appears, click [Continue Anyway].

The printer driver installation starts.

- To stop installation of the selected driver, click [Cancel] before installation is complete.

- A user code can be set after the printer driver installation. For information about user code, see the printer driver Help.

- Auto Run may not work with certain operating system settings. In that case, launch "Setup.exe" on the CD-ROM root directory.