| ManualsContentsPreviousNext |

# Programming Initial Set Up of a Special Sender

This section describes how to program Initial Set Up of a Special Sender.

Program the “Initial Set Up” of a Special Sender. You can also specify the Bypass Tray Paper Size.

1. Press [Facsimile Features].

2. Press [Reception Settings].

3. Press [Program Special Sender].

4. Press [Initial Set Up].

5. Select the function you want to program.

6. To program Authorized Reception and Special Reception Function, press [Authorized Reception] or [Special Reception Function].

7. Press [On] or [Off], and then press [OK].

   The illustration shows the “Authorized Reception” display as an example.

8. To program Bypass Tray Paper Size, press [Bypass Tray Paper Size].

9. Select the size you want to program.

   You can select a size from [Regular Size], or [Custom Size].

   If you select [Regular Size], proceed to step 10.

   If you select [Custom Size], proceed to step 11.

10. Select the size you want to program from the sizes shown.

    After selecting the size, proceed to step 14.

11. Make sure that [Vertical] is selected.

12. Enter the vertical size of the paper using the number keys, and then press [].

    Specify a vertical size from 140 mm (5.6 inches) to 900 mm (35.4 inches).

    Each time you press [mm] or [inch], the units switch between “mm” and “inch”.

    If you enter a length and change the units by pressing [mm] or [inch], it is converted automatically (fractions are rounded off).

13. Enter the horizontal size of the paper using the number keys, and then press [].

    Specify a horizontal size from 64 mm (2.6 inches) to 216 mm (8.5 inches).

    Each time you press [mm] or [inch], the units switch between “mm” and “inch”.

    If you enter a length and change the units by pressing [mm] or [inch], it is converted automatically (fractions are rounded off).

14. Press [OK].

15. Press [Exit].

16. Press the [User Tools/Counter] key.