ManualsContentsPreviousNext
Settings

# Sending over a Fax Line (Fax Destinations)

This section explains how to enter a fax number.

Use the number keys on the right side of the control panel to enter numbers.

Make sure that [Fax] is selected.

Enter the fax number using the number keys.

If you make a mistake, press the [Clear/Stop] key, and then enter again.

When adding a destination, pressing the transmission type tab switches the transmission type between fax/IP-Fax, Internet Fax, e-mail, and folder.

Press the [Start] key.

The machine starts to scan the original and stores it in memory. When scanning ends, the Communicating indicator lights and transmission starts.

- To select a destination from the Address Book, see “Using the Address Book to Specify Destinations”.

- You can insert pauses and tones in a fax number. For details, see “Entering a pause” or “Entering a tone”.

- Press [Prg. Dest.] after entering the fax number to store the fax number in the destination list. For details about storing numbers you entered, see “Registering Entered Destinations to the Address Book”.

- For the maximum number of digits that can be included in a destination, see “Maximum Values”.

- Entering a pause

- Entering a tone

- Using the Address Book to Specify Destinations

- Registering Entered Destinations to the Address Book

- Maximum Values

Related topics

Entering a pause
Entering a tone