| ManualsContentsPreviousNext |

# LAN-Fax Driver

This section describes the file path and system requirements of the LAN-Fax driver.

- You can install the LAN-Fax driver from the CD-ROM provided with this machine or download it from the manufacturer's Web site.

This driver is required to use LAN-Fax functions.

File path

The driver is included in the following folder on the CD-ROM:

`\DRIVERS\LAN-FAX\XP_VISTA`

System requirements

- Hardware

  PC/AT-compatible machines that support the following operating system properly

- Operating systems

  Windows XP/Vista/7

  Windows Server 2003/2003 R2/2008/2008 R2

- Display

  VGA 640 × 480 pixels or more

- Before beginning installation, exit all other applications.