| ManualsContentsPreviousNext |

# set

Use the "set" command to set the protocol information display "up" or "down".

View settings

The following command displays the protocol information (up/down).

`msh> set ipv4`

`msh> set ipv6`

`msh> set ipsec`

`msh> set netware`

- This command is available only when the NetWare is installed.

`msh> set smb`

`msh> set protocol`

- When protocol is specified, information about TCP/IP, NetWare and SMB appears.

`msh> set lpr`

`msh> set lpr6`

`msh> set ftp`

`msh> set ftp6`

`msh> set rsh`

`msh> set rsh6`

`msh> set diprint`

`msh> set diprint6`

`msh> set web`

`msh> set snmp`

`msh> set ssl`

`msh> set ssl6`

`msh> set nrs`

`msh> set rfu`

`msh> set rfu6`

`msh> set ipp`

`msh> set ipp6`

`msh> set http`

`msh> set http6`

`msh> set bonjour`

`msh> set bonjour6`

`msh> set nbt`

`msh> set ssdp`

`msh> set ssh`

`msh> set sftp`

`msh> set sftp6`

`msh> set wsdev`

`msh> set wsdev6`

`msh> set wsprn`

`msh> set wsscn`

`msh> set rhpp`

`msh> set rhpp6`

`msh> set lltd`

Configuration

- Enter "up" to enable the protocol, and enter "down" to disable the protocol.

You can set the protocol to "active" or "inactive".

`msh> set ipv4 {up|down}`

- If you disable IPv4, you cannot use remote access after logging out. If you did this by mistake, you can use the control panel to enable remote access via IPv4.

- Disabling IPv4 also disables lpr, ftp, rsh, diprint, web, snmp, ssl, ipp, http, bonjour, wsdev, and sftp.

`msh> set ipv6 {up|down}`

- If you disable IPv6, you cannot use remote access after logging out. If you did this by mistake, you can use the control panel to enable remote access via IPv6.

- Disabling IPv6 also disables lpr6, ftp6, rsh6, diprint6, ssl6, ipp6, http6, bonjour6, wsdev6, and sftp6.

`msh> set ipsec {up|down}`

`msh> set netware {up|down}`

- This command is available only when the NetWare is installed.

`msh> set smb {up|down}`

`msh> set lpr {up|down}`

`msh> set lpr6 {up|down}`

`msh> set ftp {up|down}`

`msh> set ftp6 {up|down}`

`msh> set rsh {up|down}`

`msh> set rsh6 {up|down}`

`msh> set diprint {up|down}`

`msh> set diprint6 {up|down}`

`msh> set web {up|down}`

`msh> set snmp {up|down}`

`msh> set ssl {up|down}`

`msh> set ssl6 {up|down}`

- If Secured Sockets Layer (SSL, an encryption protocol) function is not available for the printer, you cannot use the function by enabling it.

`msh> set nrs {up|down}`

`msh> set rfu {up|down}`

`msh> set rfu6 {up|down}`

`msh> set ipp {up|down}`

`msh> set ipp6 {up|down}`

`msh> set http {up|down}`

`msh> set http6 {up|down}`

`msh> set bonjour {up|down}`

`msh> set bonjour6 {up|down}`

`msh> set ssh {up|down}`

`msh> set ssdp {up|down}`

`msh> set nbt {up|down}`

`msh> set sftp {up|down}`

`msh> set sftp6 {up|down}`

`msh> set wsdev {up|down}`

`msh> set wsdev6 {up|down}`

- If "wsdev" and "wsdev6" are enabled simultaneously, both appear as "up" on the protocol information display, but both use IPv4 for WSD (Device), WSD (Printer) and WSD (Scanner).

`msh> set wsprn {up|down}`

`msh> set wsscn {up|down}`

`msh> set rhpp {up|down}`

`msh> set rhpp6 {up|down}`

`msh> set lltd {up|down}`