| ManualsContentsPreviousNext |

# Having incoming documents printed on paper from the bypass tray

You can print documents sent from Specified Senders on paper from the bypass tray.

In “Program Special Sender” in the Facsimile Features menu, set as follows:

- Program a special sender and select the Bypass Tray for the paper tray type.

- Turn on the “Special Reception Function” in “Initial Set Up”.

- Specify a paper size in “Bypass Tray Paper Size” in “Initial Set Up”.

For details about Program Special Sender, see “Special Senders to Treat Differently”.

- You can load a maximum of 100 sheets of standard paper in the bypass tray.

- You can use a size of paper not loaded in the paper tray(s) in the bypass tray.

- When you load paper in the bypass tray, specify the paper size. The sizes that can be specified as the standard sizes are: A4, A5, B5 JIS (81/2 × 14, 81/2 × 13, 81/2 × 11, 81/4 × 13, 8 × 13, 51/2 × 81/2, 16K). When you load any other size, specify the paper size in “Custom Size”. However, if the size of the paper on the bypass tray does not match the specified paper size, a message will appear on the display prompting you to load paper of the specified size. When you have loaded the paper, press [Exit] to print the document.

- Documents printed on paper smaller than A4 may be shortened, or split across sheets.

- Paper longer than 900 mm (35.43 inches) may be creased, not sent, or jam.

- Print area depends on optional expansion memory, resolution, and vertical length of originals.

- If you use this function, Image Rotation and 180-degree rotating printing are not possible.

- Special Senders to Treat Differently