| ManualsContentsPreviousNext |

# Setting Custom Size Paper Using the Control Panel

Follow the procedure below to set the machine using the control panel when loading custom size paper onto the bypass tray.

- If you select [Machine Setting(s)] in [Bypass Tray] under [Tray Setting Priority] in [System] of [Printer Features], the settings made using the control panel have priority over the printer driver settings. For details about [System] settings, see "System".

1. Press the [User Tools/Counter] key on the control panel.

2. Press [System Settings].

3. Press the [Tray Paper Settings] tab.

4. Press [Printer Bypass Paper Size].

5. Press [Custom Size].

   If a custom size is already set, press [Change Size].

6. Press [Vertical], enter the vertical size of the paper using the number keys, and then press [].

7. Press [Horizontal], enter the horizontal size of the paper using the number keys, and then press [].

8. Press [OK].

   The paper sizes entered are displayed.

9. Press [OK].

10. Press the [User Tools/Counter] key.

    The initial screen appears.

- When loading thick paper, thin paper or OHP transparencies, set paper size and paper type.

- The default paper size for the bypass tray is as follows:

  - (mainly Europe and Asia)

    A4

  - (mainly North America)

    81/2 × 11

- For details about setting printer drivers, see the printer driver Help.

- System