ManualsContentsPreviousNext
Settings

# authfree

Use the "authfree" command to view and configure authfree parameters.

View settings

The following command displays the current authfree settings:

`msh> authfree`

- If print job authentication exclusion is not set, authentication exclusion control cannot be displayed.

IPv4 address settings

`msh> authfree "ID" range_addr1 range_addr2`

IPv6 address settings

`msh> authfree "ID" range6_addr1 range6_addr2`

IPv6 address mask configuration

`msh> authfree "ID" mask6_addr1 masklen`

USB settings

`msh> authfree usb [on|off]`

- To enable authfree, set to on. To disable authfree, set to off. Always specify the interface.

Authentication exclusion control initialization

`msh> authfree flush`