ManualsContentsPreviousNext
Settings

# Adjusting the Volume

This section describes how to adjust the volume.

You can change the volume of the following sounds that the machine makes.

On Hook Mode

Heard when [On Hook] is pressed.

At Transmission

Heard when "Immediate Transmission" is performed.

At Reception

Heard when the machine receives a document.

At Dialing

Heard after pressing the [Start] key, until the line connects to the destination.

At Printing

Heard when a received document is printed.

Press the [User Tools/Counter] key.

Press [Facsimile Features].

Check that [General Settings] screen appears.

Press [Adjust Sound Volume].

Press [Lower] or [Louder] to adjust the volume, and then press [OK].

You can hear the actual volume by pressing [Check].

If you press [Cancel], the volume setting is canceled. The screen returns to that of step 4.

You can set the volume level to between 0 and 7.

Press the [User Tools/Counter] key.

The standby screen appears.

- You can adjust the On Hook volume when you press [On Hook]. See "On Hook Dial", Facsimile Reference.