ManualsContentsPreviousNext
Settings

# System Log Information

Use the following command to display the system log information:

- UNIX: Use the "syslog" parameter and the "rsh", "rcp", "ftp", and "sftp" commands. "rsh" and "rcp" cannot be used in a Windows environment.

- telnet: Use the "syslog" command.

Message | Problem and solutions
--- | ---
Access to NetWare server <file server name> denied. Either there is no account for this print server on the NetWare server on the password was incorrect. | Login to the file server failed when the print server was online. Make sure the print server is registered in <file server name>. If a password is specified for the print server, delete the password.
account is unavailable: same account name be used. | User account is disabled. This could be because it use the same account name as the administrator account.
account is unavailable: The authentication password is not set up. | User account is disabled. This could be because the authentication password is not set, and only the encryption account is set.
account is unavailable: encryption is impossible. | Encryption is not possible and account is disabled. This could be because: Security option is not installed. Encryption password has not been specified.
add_sess_IPv4: bad trap addr: <IPv4 address>, community: <community name> | The IPv4 address (0.0.0.0) is unavailable when the community access type is TRAP. Specify the host IPv4 address for the TRAP destination.
add_sess_IPv4: community <community name> already defined. | The same community name already exists. Use another community name.
add_sess_IPv6: bad trap addr: <IPv6 address>, community: <community name> | The IPv6 address [::] is unavailable when the community access type is TRAP. Specify the host IPv6 address for the TRAP destination.
add_sess_IPv6: community <community name> already defined. | The same community name already exists. Use another community name.
add_sess_IPX: bad trap addr: <IPX address> community <community name> | The IPX address (00:00:00:00:00:00) is unavailable when the community access type is TRAP. Specify the host IPX address for the TRAP destination.
add_sess_IPX: community <communityname> already defined. | The same community name already exists. Use another community name.
adjust time server <NTP server name> offset: xx sec. | ncsd tells you the timing of the NTP server and whether or not the time system clock is set. NTP Server: NTP server name offset: number of seconds of delay (minus number if a time in advance is specified)
Attach FileServer=<file server> | Connection to the file server as the nearest server has been established.
Attach to print queue <print queue name> | The system connects to the print queue when the print server goes online.
authenticated | The supplicant has been authenticated. Authentication was successful. When authentication is successful, this message always appears at the end of the process.
authenticating | The supplicant is authenticating with the access point (EAP or WPA).
authentication mode mismatch | The authentication mode of the access point is different from the authentication mode of the supplicant. Use the same authentication mode between the access point and the supplicant.
child process exec error ! (process name) | The network service failed to start. Turn the machine off and then on. If this does not work, contact your service or sales representative.
cipher suite mismatch | The uni-cast / multi-cast suite (TKIP/AES/WEP) of the access point is different from the suite used by the supplicant.
client EAP method rejected | The authentication mode of the access point is different with the authentication mode of the supplicant. Use the same authentication mode between the access point and the supplicant.
client password rejected | The client's password was rejected. Check the client password.
client TLS certificate rejected | The client's TLS certificate was rejected. Check the certificate.
Connected DHCP server <DHCP server address> | The IP address was successfully received from the DHCP server.
Connected DHCPv6 server <IPv6 address> | The IP address was successfully received from the DHCPv6 server.
connecting | The supplicant is establishing the Wireless LAN connection with the access point.
connection from <IP address> | A user logged in from the host <IP address>.
Could not attach to FileServer <error number> | Connection to the file server could not be established when the remote printer went online. The file server refused the connection for unknown reason. Check the file server's configuration.
Could not attach to PServer <print server> | Connection to the print server has not been established when the remote printer is turned on. The print server has refused the connection. Check the print server configuration.
Current Interface Speed: xxx Mbps | Speed of the network (10Mbps, 100 Mbps, or 1Gbps).
Current IP address (<current IP address>) | The IP address <current IP address> was acquired from the DHCP server.
Current IPX address <IPX address> | The current IP address is <IPX address>.
dpsd is disabled. | Communication via PictBridge is unavailable because PictBridge is disabled in the security mode. Enable PictBridge in the security mode.
DHCP lease time expired. | The DHCP lease time has expired. Perform the DHCP discover again. The IP address you have been using is no longer available.
DHCP server not found. | The DHCP server was not found. Make sure that the DHCP is on the network.
DHCPv6 server not found. | The DHCPv6 server was not found. Make sure that the DHCPv6 is on the network.
disconnected | The supplicant has no connection.
Duplicate IP=<IP address>(from <MAC address>). | A conflicting IPv4 or IPv6 address was used. Each IPv4 or IPv6 address must be unique. Check the device address in [MAC address].
Established SPX Connection with PServer, (RPSocket=<socket number>, connID=<connection ID>) | Connection to the print server was established when the remote printer went online.
exiting | The LPD service has completed and the process is exiting.
Exit pserver | (In the print server mode) The print server function is disabled because the necessary print server settings have not been made.
Frametype=<frametype name> | The specified frame type name <frame type name> is for NetWare use.
httpd start. | The httpd has started.
IEEE 802.11 Card does NOT support WPA. | A wireless card that does not support WPA is installed. Install a wireless card that supports WPA.
IEEE 802.11 Card Firmware REV.<version> | Displays the version number of the 802.11 card's firmware.
IEEE 802.11 current channel <channel number> | Displays the current channel number of the active wireless card (in ad hoc and infrastructure mode).
IEEE 802.11 MAC Address = <MAC address> | Displays the MAC address of the wireless interface.
IEEE 802.11 SSID <ssid> (AP MAC Address <MAC address>) | The MAC address and SSID of the access point are connected in infrastructure mode.
IEEE 802.11 <communication mode> mode | Displays the IEEE 802.11 communication mode.
(IKE phase-1) mismatched authentication type: local=<authentication type 1> remote=<authentication type 2> | This machine's <authentication type 1> in IKE phase 1 does not match the communicating host's <authentication type 2>. Make sure this machine's ISAKMP SA authentication type matches that of the communicating host.
(IKE phase-1) mismatched encryption type: local=<encryption algorithm 1> remote=<encryption algorithm 2> | This machine's ISAKMP SA Oakley group <encryption algorithm 1> in IKE phase 1 does not match the communicating host's ISAKMP SA Oakley group < encryption algorithm 2>. Make sure this machine's ISAKMP SA Oakley group matches that of the communicating host.
(IKE phase-1) mismatched DH group: local=<DH group number 1> remote=<DH group number 2> | This machine's ISAKMP SA Oakley group <DH group number 1> in IKE phase 1 does not match the communicating host's ISAKMP SA Oakley group <DH group number 2>. Make sure this machine's ISAKMP SA Oakley group matches that of the communicating host.
(IKE phase-1) mismatched hash type: local=<Hash Algorithm 1> remote=<Hash Algorithm 2> | This machine's ISAKMP SA <Hash Algorithm 1> in IKE phase 1 does not match the communicating host's ISAKMP SA <Hash Algorithm 2>. Make sure this machine's ISAKMP SA Hash Algorithm matches that of the communicating host.
IKE [% s] is disable, set PSK text. | The specified IKE entry invalid. Enter the PSK text.
inetd start. | The inetd service has started.
Interface (interface name): Duplicate IP Address (<IP address>). | The same IP (IPv4 or IPv6) address was used. Each IP address must be unique. Check the address of the device indicated in [IP address].
<Interface name> card removed | The interface managed by the supplicant has been removed.
<Interface name> interface down | The interface managed by the supplicant is disabled, or cannot connect to the access point.
<Interface name> interface up | The interface managed by the supplicant is enabled, or is connected to the access point.
< Interface > started with IP: < IP address > | IP address (IPv4 or IPv6 address) has been set for the interface and is operating.
< Interface >: Subnet overlap. | The same IP address (IPv4, or IPv6 address) and the subnet mask is used with other device.
IPP cancel -job: permission denied. | The spooled job was canceled due to error or user request.
IPP job canceled. jobid=%d. | The spooled job was canceled due to error or user request.
job canceled. jobid=< job ID > | The spooled job was canceled due to error or user request.
LEAP challenge to access point failed | The LEAP challenge to the access point has failed.
LeaseTime=<lease time>(sec), RenewTime=<renew time>(sec). | The resource lease time received from the DHCP server is displayed in [lease time] in seconds. The renewal time is displayed in [renew time] in seconds.
Login to fileserver <file server name> (<IPX|IP>), <NDS|BINDERY> | When the print server was online, the system logged in to <file server> in NDS or BINDERY mode. The transfer protocol in use is also displayed.
Manual [%s] is disable, set authentication key. | The specified manual SA entry is invalid. Set the authentication key.
Manual [%s] is disable, set encryption key. | The specified manual SA entry is invalid. Set the authentication key.
Memory allocate error. | Date cannot be obtained. Disconnect the USB cable, and then connect it.
MIC failure TKIP counter measures started | The supplicant using TKIP has detected two instances of tampering within 60 seconds and has started counter measures.
MIC failure TKIP counter measures stopped | Counter measures have stopped after 60 seconds (since the supplicant using TKIP started counter measures against tampering).
Name registration failed. name=<NetBIOS name> | Name registration of <NetBIOS Name> failed. Change to a different NetBIOS name.
Name registration success in Broadcast name=<NetBIOS name> | Name registration by <NetBIOS Name> broadcast was successful.
Name registration success. WINS server=<WINS server address> NetBIOS Name=<NetBIOS name> | Name registration of <NetBIOS Name> to <WINS server address> was successful.
nbtd start. | The nbtd (NetBIOS over TCP/IP Daemon) has started.
no RADIUS/authentication server | The supplicant has received a message reporting that a usable RADIUS server cannot be found.
no smart card detected on device | PEAP/GTC (Generic Token Card) is selected, but a smart card using GTC authentication cannot be found.
no SSID in scan result | A network with the SSID you specified was not found. The specified SSID might not be available, or the signal from the access point/multi-channel might be weak.
no WPA information element in probe response, rescanning | There is no WPA information on the response from the SSID probe of the access point you want to use. The supplicant is rescanning.
npriter start. (NetWare) | (In the remote printer mode) The NetWare service has started.
nwstart start. (NetWare) | The NetWare protocol stack setup server has started.
Open log file <file name> | The specified log file was opened when the print server was online.
permission denied. | When canceling a job, it was determined after checking the user name and host address that the user's privileges were insufficient. (Does not apply to root privileges.)
Printer <printer name> has no queue | The print queue is not assigned to the printer when the print server was online. Assign the print queue to the printer using NetWare administrator account, and then restart the printer.
Print queue <print queue name> cannot be serviced by printer 0, <print server name> | The print queue cannot be established when the print server is online. Make sure that the print queue exists on the specified file server.
Print server <print server name> has no printer | The printer was not assigned to the print server when the print server was online. Use the NetWare administrator account to assign the printer, and then restart the printer.
print sessions full | No more print jobs can be accepted. Wait a while before sending any more print jobs.
pserver start. (NetWare) | NetWare service has started in print server mode at the print server operation.
Required file server (<file server name>) not found | The required file server <file server name> could not be found.
restarted. | The LPD has started.
sap enable. saptype=<SAP type>, sapname=<SAP name> | The SAP function was started. The SAP packet is issued to advertise the service in the SAP table on the NetWare server.
server certificate invalid | The server ID is disabled. Check the server authentication.
server identity invalid | The server ID is disabled. Check the server authentication.
server not trusted | The RADIUS server cannot be trusted.
session_IPv4 <community name> not defined. | The requested community name is not defined.
session_IPv6 <community name> not defined. | The requested community name is not defined.
session_IPX <community name> not defined. | The requested community name is not defined.
Set context to <NDS context name> | The NDS context name <NDS context name> has been set.
shutdown signal received. network service rebooting... | The network is rebooting.
smbd start. (NetBIOS) | SMBD (Server Message Block Daemon) has been started.
SMTPC: failed to connect smtp server. | Connection to the SMTP server failed. This could be because no connection to the network has been established, or the network configuration is incorrect, so there is no response from the SMTP server, or the specified SMTP server name is incorrect, or the specified SMTP server IP address could not be found in the DNS server, or a server other than the SMTP server has been specified, or the specified SMTP server port number is incorrect. Check the DNS Server's IP address and SMTP server's IP address, or the SMTP server name and SMTP port number, or the SMTP server's SMTP port number, or the network connection and configuration.
SMTPC: failed to connect smtp server. timeout. | Connection to the SMTP server failed due to timeout. This could be because the specified SMTP server name is incorrect, or no connection to the network has been established, or the network configuration is incorrect, so there is no response from the SMTP server. Check the SMTP server name, or the network connection and configuration.
SMTPC: failed to get smtp server ip-address. | The SMTP server IP address could not be obtained. This could be because: The specified DNS server could not be found. No connection to the network has been established. An incorrect DNS server is specified. The specified SMTP server IP address could not be found in the DNS server.
SMTPC: no smtp server. connection close. | Connection to the SMTP server failed due to no response from SMTP. This could be because a server other than the SMTP server has been specified, or the specified SMTP server port number is incorrect. Check the SMTP server name, port number, or the SMTP server port number.
SMTPC: refused connect by smtp server. | Connection to the SMTP server is denied. This could be because server other than the SMTP server has been specified, or the specified SMTP server port number is incorrect. Check the SMTP server name, port number, or the SMTP server port number.
SMTPC: username or password wasn't correct. [response code] (information) | Connection to the SMTP server failed, because the specified SMTP user name is incorrect, or the specified SMTP password is incorrect. Check the SMTP user name and password.
Snmp over IPv4 is ready. | Communication over IPv4 with snmp is available.
Snmp over IPv6 is ready. | Communication over IPv6 with snmp is available.
Snmp over IPX is ready. | Communication over IPX with snmp is available.
Snmpd Start. | The snmpd has started. This message is displayed only when the power is turned on.
started. | The direct printing service has started.
started. | The IKE service has started.
Started. | The bonjour (rendezvous) function has started.
stopped | The supplicant has just stopped.
success key received | The supplicant received the EAP-Success key.
success but invalid key | The supplicant received a message reporting that EAP authentication was successful, but the EAPOL key was invalid.
supplicant started | The supplicant has just started.
supplicant unbound | The supplicant is not connected to the unbound access point.
terminated. | The IKE service has stopped because no configurations for manual SA or IKE exist.
Terminated. | The bonjour (rendezvous) function is disabled.
There is problem in dhcp server operation. | There is a problem with the DHCP server. If multiple DHCP servers are active on the network, check that they are assigning unique IP addresses to each machine.
The print server received error <error number> during attempt to log in to the network. Access to the network was denied. Verify that the print server name and password are correct. | Login to the file server failed when the print server was online. The print server is not registered or a password is specified. Register the print server without specifying a password.
trap account is unavailable. | v3Trap cannot be sent. This could be because the Trap destination account is different from the account specified by the machine.
unauthenticated | The authentication failed. The supplicant was denied access to the access point, or was not authenticated.
Updated (option name)(value) via DHCPv6 Server | The parameter obtained from the DHCP server has been updated.
usbd is disabled. | Plug and Play is unavailable because the machine is in Security Mode. Enable USBD in Security Mode.
waiting for keys | The supplicant is waiting for the session key.
WINS name registration: No response to server (WINS server address) | There was no response from the WINS server. Check that the correct WINS server address is entered. Also, check that the WINS server is functioning properly.
WINS wrong scopeID=<scope ID> | The scope ID is invalid. Use a valid scope ID.
write error occurred. (diskfull) | A "diskfull" error occurred while the machine was writing to the spool file. Wait for the current print job to finish. When it finishes, more HDD space will be available. Only pages that were spooled when the error occurred will be printed.
write error occurred. (fatal) | A "fatal" error occurred while the machine was writing to the spool file. Wait for the current print job to finish. When it finishes, more HDD space will be available. Only pages that were spooled when the error occurred will be printed.
WSD (Device) started. | WSD (Device) has started.
WSD (Printer) started. | WSD (Printer) has started.
WSD (Scanner) started. | WSD (Scanner) has started.

- For details about UNIX commands and parameters, see UNIX Supplement.