| ManualsContentsPreviousNext |

# Printer configuration

You can check the printer configuration using telnet.

This section explains the checking procedure for input/output tray and printer language.

- UNIX: Use the "info" parameter and the "rsh", "rcp", "ftp", and "sftp" commands. "rsh" and "rcp" cannot be used in a Windows environment.

- telnet: Use the "info" command.

Input Tray
Item | Description
--- | ---
No. | ID number of the paper tray
Name | Name of the paper tray
Paper Size | Size of paper loaded in the paper tray
Status | Current status of the paper tray Normal: Normal NoInputTray: No tray PaperEnd: No paper

Output Tray
Item | Description
--- | ---
No. | ID number of the output tray
Name | Name of the output tray
Status | Current status of the output tray Normal: Normal PaperExist: Paper exist OverFlow: Paper is full Error: Other errors

Printer Language
Item | Description
--- | ---
No. | ID number of the printer language used by the machine
Name | Name of the printer language used in the machine
Version | Version of the printer language

- For details about UNIX commands and parameters, see UNIX Supplement.