| ManualsContentsPreviousNext |

# Current Machine Status

This section explains how you can check the machine's status and the items displayed. Depending on the options installed on the machine, some items might not be displayed.

- UNIX: Use the "stat" parameter and the "rsh", "rcp", "ftp", and "sftp" commands. "rsh" and "rcp" cannot be used in a Windows environment.

- telnet: Use the "status" command.

Messages | Description
--- | ---
Access Restricted | The job was canceled because user have no authority.
Call Service Center | There is a malfunction in the machine.
Canceled | The job is reset.
Canceling Job... | The job is being reset.
Cannot Eject Original Through | The original cannot be ejected.
Change Tnr Cartridge to Stndard | Replace the toner cartridge with the standard toner cartridge.
Change Toner Cartridge to MICR | Replace the toner cartridge with the MICR toner cartridge.
Configuring... | Setting is being changed.
Cover Open: ADF | The document feeder is open.
Cover Open: Duplex Unit | The cover of the duplex unit is open.
Cover Open: Finisher | The cover of Finisher is open.
Cover Open: Front Cover | The front cover is open.
Cover Open: Rear Cover | The rear cover is open.
Data Size Error | The data size error occurred.
Error | An error has occurred.
Error: Address Book | An error has occurred in the data of the address book.
Error: Command Transmission | An error has occurred in the machine.
Error: Ethernet Board | An Ethernet board error has occurred.
Error: HDD Board | A hard disk drive board error has occurred.
Error: Media Link Board | An error has occurred on the File Format Converter.
Error: Memory Switch | A memory switch error has occurred.
Error: Optional Font | An error has occurred in the font file of the machine.
Error: PDL | An error has occurred in the page description language.
Error: Rem. Certificate Renewal | An error has occurred in the remote server renewal.
Error: USB Board | An error has occurred in the USB interface board.
Error: USB Interface | An error has occurred in the USB interface.
Error: Wireless Board | An error has occurred in the wireless interface board or IEEE 802.11 interface unit.
Error: Wireless Card | Wireless card is not inserted during start up, or the IEEE 802.11 interface unit or the wireless card is taken out after start up.
Exceed Stapling Limit | The printing has exceeded the stapling limit.
Full: Finisher Shift Tray | Shift tray of Finisher is full.
Full: Internal Tray 1 | The internal tray 1 is full.
Hex Dump Mode | It is a hex dump mode.
Immed. Trans. not connected | It did not connect directly with the other party of the transmission.
Immediate Transmission Failed | An error has occurred while transmitting directly.
In Use: Copier | The copier is being used.
In Use: Fax | The fax is being used.
In Use: Finisher | Other functions is using Finisher.
In Use: Input Tray | Other functions is using the input tray.
In Use: Staple Unit | Other functions is using the staple unit.
Independent-supplier Toner | Toner that is not recommended is set.
Jobs Suspended | All jobs are suspended.
Key Card not inserted | The machine is waiting for the key card to be inserted.
Key Counter not inserted | The machine is waiting for the key counter to be inserted.
Malfunction: Finisher | There is a problem with the finisher.
Malfunction:Lower Paper Tray(s) | There is a problem with the bank motor.
Malfunction: Output Tray | There is a problem with the output tray.
Malfunction: Staple Unit | There is a problem with the staple unit.
Memory Low: Copy | Memory shortage has occurred while the copy was operating.
Memory Low: Data Storage | Memory shortage has occurred while the document was being accumulated.
Memory Low: Fax Scanning | Memory shortage has occurred while transmitting the fax.
Memory Low: Scanning | Memory shortage has occurred while the scanner was working.
Miscellaneous Error | Other error has occurred.
Mismatch: Paper Size | Indicated paper tray does not contain paper of selected size.
Mismatch: Paper Size and Type | Indicated paper tray does not contain paper of selected size and type.
Mismatch: Paper Size/Image Size | Indicated paper tray does not contain paper that matches the size of the print image.
Mismatch: Paper Type | Indicated paper tray does not contain paper of selected type.
Near Replacing: Maintenance Kit | Prepare a new maintenance kit.
Need more Staples | Stapler has almost run out of staples.
No Paper: Selected Tray | There is no paper in specified tray.
No Paper: Tray 1 | There is no paper in tray 1.
No Paper: Tray 2 | There is no paper in tray 2.
No Paper: Tray 3 | There is no paper in tray 3.
No Paper: Tray 4 | There is no paper in tray 4.
Not Detected: Finisher | The finisher is not correctly set.
Not Detected: Fusing Unit | The fusing unit is not correctly set.
Not Detected: Input Tray | The paper feed tray is not correctly set.
Not Detected: Tray 1 | Tray 1 is not correctly set.
Not Detected: Tray 2 | Tray 2 is not correctly set.
Not Detected: Tray 3 | Tray 3 is not correctly set.
Not Detected: Tray 4 | Tray 4 is not correctly set.
Not Detected: Print Cartridge | Print cartridge is not correctly set.
Not Reached, Data Deleted | Unreached job is deleted.
Not Reached, Data Stored | Unreached documents are saved.
Nr Replcng: Prt Cart Bk Tnr Low | Toner is almost running out. Prepare a new print cartridge.
Nr Repl: Prt Crt Pt Life End Sn | The life of the photoconductor unit is almost ending. Prepare a new print cartridge.
Offline | Machine is offline.
Original on Exposure Glass | The original remains on the exposure glass.
Panel Off Mode | The machine is in Panel-Off mode.
Panel Off Mode>>Printing ava. | The machine is in Control Panel-Off mode.
Paper in Duplex Unit | The paper remains in the duplex unit.
Paper in Finisher | The paper remains in Finisher.
Paper Misfeed: ADF | The paper has jammed in Document Feeder.
Paper Misfeed: Duplex Feed Unit | The paper has jammed in Duplex Unit.
Paper Misfeed: Finisher | The paper has jammed in Finisher.
Paper Misfeed: Input Tray | The paper has jammed in the input tray.
Paper Misfeed: Internal Path | The paper has jammed inside the machine.
Paper Misfeed: Optional Tray 1 | The paper has jammed in the first tray of the paper feed unit.
Paper Misfeed: Optional Tray 2 | The paper has jammed in the second tray of the paper feed unit.
Paper Misfeed: Optional Tray 3 | The paper has jammed in the third tray of the paper feed unit.
Print Complete | The print was completed.
Printing... | Printing is in progress.
Processing | Data is being processed.
Proxy User/Password Incorrect | The proxy user name and password setting is incorrect.
RC Gate Connection Error | Failed connect with RC Gate.
Ready | The machine is ready to print.
Renewing Remote Certificate | The remote certificate is being renewed.
Replace Maintenance Kit | It is time to replace the maintenance kit.
Replace Prt Crtdg: Bk Tnr Empty | Toner has run out. It is time to replace the print cartridge.
Replace Prt Crtdg: Wst Tnr Full | The waste toner is full. It is time to replace the print cartridge.
Replace Prt Cart: Pt Life Ended | The life of the photoconductor unit has ended. It is time to replace the print cartridge.
SD Card Authentication failed | SD card authentication failed.
Setting Remotely | The RDS setting is being processed.
Skipped due to Error | Skipped the error.
Storage Complete | The storage is complete.
Storage Failed | The storage has failed.
Supplies Order Call failed | The supply order call has failed.
Transmission Aborted | The transmission was interrupted.
Transmission Complete | The transmission completion was completed.
Transmission Failed | The transmission has failed.
Tray Error: Chaptering | The paper feed tray specification error has occurred because chaptering as well as the normal paper use the same tray for printing.
Tray Error: Duplex Printing | Selected paper tray cannot be used for duplex printing.
Unit Left Open: ADF | Document feeder is opened.
Waiting for Job Suspension | The machine is waiting for Job Suspension.
Warming Up... | The machine is warming up.

- For details about UNIX commands, see UNIX Supplement.

- Check the error contents that may be printed in the configuration page.