| ManualsContentsPreviousNext |

# Selecting Type of Transmission

You can select the transmission type: standard fax, IP-Fax, Internet Fax, e-mail transmission, or folder transmission.

Press the tab in the standby display to select the transmission type.

When sending to a standard fax or IP-Fax destination

Make sure that [Fax] is selected.

When sending to an Internet Fax destination

Press [Internet Fax] to switch the type of transmission to Internet Fax.

When sending to an e-mail destination

Press [E-mail] to switch the type of transmission to e-mail.

When sending to a folder destination

Press [Folder] to switch the type of transmission to folder.

- For details about each transmission type, see “IP-Fax Functions”, “Internet Fax Transmission”, “E-mail Transmission”, and “Folder Transmission”.

- IP-Fax Functions

- Internet Fax Transmission

- E-mail Transmission

- Folder Transmission