| ManualsContentsPreviousNext |

# Entering the path to an FTP server manually

You can enter the path to an FTP server manually.

1. Press [Manual Entry].

2. Press [FTP].

3. Press [Manual Entry] on the right side of the server name field.

   The soft keyboard appears.

4. Enter a server name.

   Instead of the server name, you can also use its IPv4 address.

5. Press [OK].

6. Press [Manual Entry] on the right side of the path field.

7. Enter the path for the folder.

   The following is an example of a path where the folder name is "user" and the subfolder name is "lib": user\lib.

8. Press [OK].

9. Enter the user name according to the setting at the destination.

   Press [Manual Entry] to the right of the user name field to display the soft keyboard.

10. Enter the password according to the setting at the destination.

    Press [Manual Entry] next to the password field to make the soft keyboard appear.

11. To change the port number which is set in [System Settings], press [Change] on the right side of the port number field. Enter a port number using the number keys, and then press the [] key.

12. Press [Connection Test].

    A connection test is performed to check whether the specified folder exists.

    If the message `"Connection with PC has failed. Check the settings."` appears, see "Troubleshooting When Using the Scanner Function", Troubleshooting.

13. Check the connection test result, and then press [Exit].

14. Press [OK].

- If you change the protocol after entering the path name, user name, or password, a confirmation message appears.

- The connection test may take time.

- You may not be able to press [Connection Test] right after pressing [Cancel] during a connection test.

- To change the registered path to a destination folder, press [Edit] to the left of the destination field to display the soft keyboard, enter the new path, and then click [OK].

- You can register the path to the destination in the machine's address book. For details, see "Registering the Path to the Selected Destination in the Address Book".

- The machine may fail to transfer the file if you do not have write privileges for the folder or there is not enough free hard disk space.

- Registering the Path to the Selected Destination in the Address Book