ManualsContentsPreviousNext
Settings

# When B is displayed

This section describes how to remove misfeeds from location “B”.

Remove any paper from the bypass tray.

Close the bypass tray.

Push the button on the right side of the machine to open the front cover.

Hold the print cartridge's front handle to lift and pull it out.

Remove the misfed paper.

Raise the lever B.

1. Lever B

Remove the misfed paper, and then lower the lever B.

Return the print cartridge to its original position.

Close the front cover.