ManualsContentsPreviousNext
Settings

# Paper Size and Scanned Area

This section explains the size of the area the machine can scan.

- There may be a difference in the size of the image when it is printed at the destination.

- Even if an original is correctly placed on the exposure glass or in the ADF, a margin of 3 mm (0.1 inches) around each edge of the original may not be sent.

Related topics

When placing an original on the exposure glass
When placing an original into the Auto Document Feeder