ManualsContentsPreviousNext
Settings

# sntp

The printer clock can be synchronized with a NTP server clock using Simple Network Time Protocol (SNTP). Use the "sntp" command to change the SNTP settings.

View settings

`msh> sntp`

NTP IPv4 server address configuration

You can specify the IPv4 address of the NTP server.

`msh> sntp server "IPv4_address"`

NTP hostname configuration

You can specify the hostname of the NTP server.

`msh> sntp server "hostname"`

Deleting NTP server configuration

`msh> sntp server clear`

Interval configuration

`msh> sntp interval "polling_time"`

- You can specify the interval at which the printer synchronizes with the operator-specified NTP server. The default is 60 minutes.

- The interval can be entered from 0, or between 15 and 10,080 minutes.

- If you set 0, the printer synchronizes with the NTP server only when you turn the printer on. After that, the printer does not synchronize with the NTP server.

Time-zone configuration

`msh> sntp timezone "±hour_time"`

- You can specify the time difference between the printer clock and NTP server clock. The values are between -12:00 and +13:00.

- You can only select either the address or host name for the ntp server.