ManualsContentsPreviousNext
Settings

# Connecting to the Ethernet Interface (mainly North America)

This section describes how to connect an Ethernet cable to the Ethernet interface.

- If the main power switch is on, turn it off.

- Use the following Ethernet cables.

  - Unshielded Twisted Pair Cable (UTP) or Shielded Twisted Pair Cable (STP) and Category type 5 or more

Make sure the main power is switched off.

Connect the Ethernet interface cable to the 10BASE-T/100BASE-TX port.

Connect the other end of the Ethernet interface cable to a network connection device such as a hub.

Turn on the main power switch of the machine.

1. Indicators

   When 100BASE-TX or 10BASE-T is operating, the green LED is lit and the orange LED flashes. If the machine is not connected to the network, both LEDs are turned off.

- For details about how to turn on the main power switch, see “Turning On/Off the Power”.

- For details about installing the printer driver, see "Preparing the Machine", Printer Reference.

- Turning On/Off the Power