ManualsContentsPreviousNext
Settings

# Optimum environmental conditions

This section describes acceptable and recommended temperature and humidity ranges of the environment where this machine will be installed.

- Temperature: 10 32 °C (50 89.6 °F) (humidity to be 54% at 32 °C, 89.6 °F)

- Humidity: 15 80% (temperature to be 27 °C, 80.6 °F at 80%)

- A strong and level base.

- The machine must be level within 5 mm, 0.2 inches: both front to rear and left to right.