| ManualsContentsPreviousNext |

# Specifying Tray for Lines

Use this function to specify the output tray for each line port.

You can specify the document feeding tray for each port (telephone, Internet Fax, IP-Fax). You can also set the machine to output Internet Fax documents and ordinary faxes onto different trays.

- This function is available on type 2 model only.

- To use this function, specify the port and destination using [Specify Tray for Lines] in the Facsimile Features menu. For details about the setting, see “Reception Settings”.

- Reception Settings