ManualsContentsPreviousNext
Settings

# Forwarding

Print received documents, and then transfer them to those receivers programmed beforehand.

It is also possible to forward faxes sent only by senders programmed as Special Senders.

- If you select [Same as Basic Settings], the fax document is forwarded to the receivers programmed in “Forwarding” under Facsimile Features.

- If you do not program any Special Senders, the machine transfers all incoming documents to the other end receivers specified in “Forwarding” under Facsimile Features.

- You can set the fax destination, Internet Fax destination, IP-Fax destination, e-mail destination, or folder destination, as a forward destination.

- If you have specified e-mail destination or folder destination for forwarding, you can specify the file format used for forwarding. See “Parameter Settings” (switch 21, bit 3).

- Parameter Settings