| ManualsContentsPreviousNext |

# Installing the PostScript 3 printer driver (TCP/IP)

1. Quit all applications currently running.

2. Insert the CD-ROM into the CD-ROM drive.

   The installer starts.

3. Select an interface language, and then click [OK].

   The printer driver with the selected language will be installed. The English printer driver is installed when the following language is selected: Suomi, Magyar, Cestina, Polski, Portugues, Russian.

4. Click [PostScript 3 Printer Driver].

   Add Printer Wizard starts.

5. Click [Next >].

6. Click [Local printer attached to this computer], and then click [Next >].

7. Click [Create a new port:].

8. Click [SmartDeviceMonitor for Client 2] in [Type of port:], and then click [Next >].

9. Click [TCP/IP], and then click [Search].

   A list of machines using TCP/IP appears.

10. Select the machine you want to use, and then click [OK].

    Only machines that respond to a broadcast from the computer appear. To use a machine not listed here, click [Specify Address], and then enter the IP address or host name of the machine.

11. Check that the name of the machine whose driver you want to install is selected, and then click [Next >].

12. Change the machine name if you want, and then click [Next >].

    Select [Yes] to configure the machine as default.

13. Specify whether or not to share the machine, and then click [Next >].

14. Specify whether or not to print a test page, and then click [Next >].

15. Click [Finish].

    If the [Hardware Installation] message appears, click [Continue Anyway].

    The printer driver installation starts.

- To stop installation of the selected driver, click [Cancel] before installation is complete.

- A user code can be set after the printer driver installation. For information about user code, see the printer driver Help.

- Auto Run may not work with certain operating system settings. In that case, launch "Setup.exe" on the CD-ROM root directory.