ManualsContentsPreviousNext
Settings

# Maximum Values

The following list contains the maximum value for each item.

Item | Standard | Expansion memory (Optional)
--- | --- | ---
Memory | 4 MB | 28 MB
Number of documents you can store in memory for Memory Transmission | 400 | 400
Number of pages you can store in memory (using A4 Standard <ITU-T 1 Chart>) | Approx. 320 | Approx. 2,240
Number of destinations you can register in the destination list | 2,000 | 2,000
Number of groups you can register | 100 | 100
Number of destinations you can register in a group | 500 | 500
Number of destinations you can specify per file | 500 | 500
Number of destinations you can specify for all files (including files in memory) | 500 | 500
Number of destinations you can search at a time using [Search Dest.] | 100 | 100
Number of recent destinations the machine can store | 10 | 10
Number of digits that can be included in a destination | 128 | 128
Number of digits for a SEP/SUB/PWD/SID Code | 20 | 20
Number of characters you can enter in the e-mail subject line | 128 | 128
Number of communication results you can check on this machine | 200 | 200
Number of communication results printed in the Journal | 50 | 50
Number of special senders you can register | 250 | 250
Number of LAN-Fax Driver transmission results you can check using Web Image Monitor on a network computer | 70 | 70
Number of documents sent from a LAN-Fax Driver that the machine can retain as files to be sent | 400 | 400
Number of destinations you can register into a Keystroke Program | 500 | 500
Number of Keystroke Programs you can register | 100 | 100
Number of characters you can enter for a program name | 20 | 20
Number of received documents you can store on the machine's hard disk | 400 | 400
Number of documents you can print at a time in [Print / Delete Stored Reception File] | 30 | 30
Number of documents you can delete at a time in [Print / Delete Stored Reception File] | 30 | 30
Number of stored documents you can specify at a time in [Select Stored File] | 30 | 30
Number of stored pages you can send in one operation in [Select Stored File] | 1,000 | 1,000
Number of stored documents you can print at a time using [Print 1st Page] | 30 | 30
Number of stored documents you can print at a time using [Print File] | 30 | 30
Number of documents you can store in the Document Server using the facsimile function | 3,000 | 3,000
Number of pages per document you can store in the Document Server | 1,000 | 1,000
Number of pages you can store in the Document Server (in total - copy function, facsimile function, printer function, and scanner function) (Using ITU-T 4 Chart) | Approx. 9,000 | Approx. 9,000
Number of destinations you can register in the Address Book of the LAN-Fax | 2,000 | 2,000
Number of destinations you can specify at once using LAN-Fax | 500 | 500

- The maximum number of pages that can be stored or transmitted may decrease depending on the contents of documents.