| ManualsContentsPreviousNext |

# Checking the Error Log

If files could not be stored due to printing errors, identify the cause of the errors by checking the error log on the control panel.

- The most recent 30 errors are stored in the error log. If a new error is added when there are 30 errors already stored, the oldest error is deleted. However, if the earliest error is a Sample Print, Locked Print, Hold Print, or Stored Print error, it is not deleted. The error is stored separately until the number of errors reaches 30.

- If the main power switch is turned off, the log is deleted.

- You cannot view [Error Log] on the simplified display.

1. Press the [Printer] key to display the printer screen.

2. Press [Error Log].

   An error log list appears.

3. Press the desired job list, and then press [Details].

   A detailed error log appears.