| ManualsContentsPreviousNext |

# When C is displayed

This section describes how to remove misfeeds from location “C”.

1. Pull up on the lever to open the rear cover.

2. Release the lock of the fusing unit.

3. Pull out the fusing unit.

4. Remove the misfed paper, and then return the fusing unit to its original position.

5. Remove the misfed paper.

6. Remove the misfed paper from the paper exit.

   - Type 1

   - Type 2

   - Type 3

7. Close the rear cover.