ManualsContentsPreviousNext
Settings

# Setting Up as a Print Server (NetWare 4.x, 5/5.1, 6/6.5)

Follow the procedure below to connect the machine as a print server using NetWare 4.x, NetWare 5/5.1, or NetWare 6 / 6.5.

- When using the printer as a print server in NetWare 4.x, NetWare 5/5.1, or NetWare 6/6.5, set it to the NDS mode.

- When using NetWare 5/5.1 or NetWare 6/6.5, set the printer as a print server.

Start Web Image Monitor.

Click [Login].

A dialog box for entering the login user name and password appears.

Enter the login user name and password, and then click [Login].

For details about the login user name and password, consult your network administrator.

The Web browser might be configured to auto complete login dialog boxes by retaining user names and passwords. This function reduces security. To prevent the browser retaining user names and passwords, disable the browser's auto complete function.

In the menu area, click [Configuration].

Under "Network", click [NetWare].

Confirm the settings, and then click [OK].

Configuration is now complete. Wait several minutes before restarting Web Image Monitor.

Click [Logout].

Quit Web Image Monitor.

- To check the configuration is correct, enter the following from the command prompt:

  `F:> USERLIST`

- If the printer works as configured, the name of the print server appears as a connected user.

- If you cannot identify the printer you want to configure, check the printer name against the configuration page printed from the printer. If no printer names appear in the list, match the frame types of IPX/SPXs for the computer and printer. Use the [Network] dialog box of Windows to change the frame type of the computer.

- For details about Web Image Monitor, see "Using Web Image Monitor".

- Using Web Image Monitor