ManualsContentsPreviousNext
Settings

# Automatic Redial

If a fax document could not be sent because the line was busy or an error occurred during transmission, redial is attempted at five-minute intervals up to five times.

If redialing fails after four redials, the machine cancels the transmission and prints a Communication Result Report or Communication Failure Report.

- If there are a large number of files stored in memory, documents might not be sent in the order they were scanned.