ManualsContentsPreviousNext
Settings

# Entering a tone

This function allows a machine connected to a pulse dialing line to send tonal signals (for example if you want to use a special service on a tone dialing line).

When you press [Tone], the machine dials the number using tonal signals.

This section explains how to use the tone function with On Hook Dial as an example.

Press [On Hook].

Enter the fax number using the number keys.

Press [Tone].

Enter the number you want to tone dial using the number keys.

Press the [Start] key, and then press [Start TX].

Transmission starts.

If you want to cancel a transmission, press the [Clear/Stop] key, and then remove the originals.

After transmission, the standby display appears.

- Certain services may be unavailable even when using Tone function.

- A tone is shown as a “T” on the display and the next numbers are dialed using tonal signals.