ManualsContentsPreviousNext
Settings

# Installing the SD Card (Optional)

This section describes how to install the optional SD card.

| Do not remove any covers or screws other than those explicitly mentioned in this manual. Inside this machine are high voltage components that are an electric shock hazard and laser components that could cause blindness. Contact your sales or service representative if any of the machine's internal components require maintenance, adjustment, or repair. Do not attempt to disassemble or modify this machine. Doing so risks burns and electric shock. Note again that exposure to the laser components inside this machine risks blindness.

| Keep SD cards out of reach of children. If a child swallows an SD card, consult a doctor immediately.

- Do not subject the card to physical shocks.

- If you want to use two or more SD cards that can be inserted in the same slot, contact your sales and service representative.

Check the contents of the package.

Turn off the main power switch, and then unplug the machine's power cord from the wall outlet.

Loosen and remove the screw, and then carefully remove the cover of the SD card slot.

If an SD card is already inserted, push and release the SD card, pinch it, and then pull it carefully out of the slot.

Carefully push in the SD card (notched corner downward and leading), until it clicks into place.

Insert the SD card in the lower slot.

Reattach the cover over the SD card. Fasten the screw to secure the cover.

- Do not touch the card while the machine is in use. It may come loose, even if pushed only slightly. The slot cover must be reattached.

- You can confirm that the browser unit was installed correctly by checking the User Tools menu. For details, see the manuals provided with the browser unit.

- If the card is not installed properly, repeat the procedure from the beginning. If it cannot be installed correctly even after reattempting installation, contact your sales or service representative.